**Launchpad Pro Side Led Access 0.2 Beta**

**You need：**

Launchpad Pro

loopMIDI Program (inside the compress file)

Ableton Live 9 (Need purchase on your own)

Max for Live 7 (Need purchase on your own)

**Tutorial：**

**First step**

Install the loopMIDI

**Second step**

Create a new virtual MIDI Port in loopMIDI



**Third Step**

Open sideled.als

Set Ableton Live's Control Surface

Like the image



**Fourth Step**

Open sideled.maxpat

Change the MIDI Setting

Options >> MIDI Setup

Set to the same as the image



**Fifth Step**

Return the the normal interface

Follow the introduction on the screen



**Sixth Step**

Back to Live

Test the result

Set as the image



Play the clip

Then you are good to go!

**If Launchpad can't get into Live mode**

Close MAX

Reset Control Surface to Launchpad Pro



If Launchpad Pro get into Live mode and display normaly

Set it back to loop MIDI

Restart from the fifth step

**Detail:**

The LED is set to E8

Can be access on any Channel